1. [1] Kamath C , El-Dasher B , Gallegos G F , et al. Density of additively-manufactured, 316L SS parts using laser powder-bed fusion at powers up to 400 W[J]. International Journal of Advanced Manufacturing Technology, 2014, 74(1-4):65-78.